AMPED WIRELESS

Model:  AV3000 Firmware Update

Updated: 4/23/2011

_______________________________________________________________________________________________________


FIRMWARE UPGRADING INSTRUCTIONS:

You may call support at 888-573-8820 at any time for questions regarding this process.

 
PLEASE DISCONNECT FROM ALL WIRELESS NETWORKS BEFORE UPGRADING FIRMWARE.
PLEASE CONNECT DIRECTLY TO THE REPEATER WITH THE INCLUDED ETHERNET CABLE. 

1.	Open your web browser and go to http://setup.ampedwireless.com 
2.	When the menu appears, click on Management (left side menu)
3.	Go to Upgrade Firmware.
4.	Click on choose file.
5.	Select the Firmware file for your product (fw-av3000_mmddyy.bin) 
6.	Click on upload.
7.           The Smart Repeater will reboot and your page will refresh when completed.
8.           Your firmware has now been updated.  You may disconnect your computer from the Smart Repeater
              and begin using it normally.

Thank you

AMPED WIRELESS SUPPORT TEAM

___________________________________________________________________________________________________________


062311 FIRMWARE RELEASE NOTES:
- Fixed TKIP security issue in Setup Wizard
- Fixed Setup Wizard and Security Page security key input length. Now supports 64 Characters
- Added Firmware version report in Upgrade Firmware menu
- Added Auto-Load Menu (Auto-DNS) enable and disable feature
	- Enables use of Static IP address and accessing the Setup Menu via a IP address 
	  instead of setup.ampedwireless.com
	- Allows user to disable the feature: 
		 - Setup page automatically loads when connection to home network is dropped


040811 FIRMWARE RELEASE NOTES:
- Fixed TKIP accessibility issue in security menu
- Added Home Network Signal Strengh display in Status Page
- Fixed left side navigation menu (removed) issue in saved settings page


