AMPED WIRELESS

Model:  R10000 Firmware Update

Firmware Version: v2.5.2.11

Updated: 12/07/2012

_______________________________________________________________________________________________________


FIRMWARE UPGRADING INSTRUCTIONS:

You may call support at 888-573-8820 at anytime for questions regarding this process.

PLEASE CONNECT YOUR COMPUTER TO THE R10000 HIGH POWER ROUTER (WIRELESS OR WIRED)

1.	Open your web browser and go to http://setup.ampedwireless.com 
2.	When the menu appears, click on More Settings then click Management (left side menu)
3.	Go to Upgrade Firmware.
4.	Click on choose file.
5.	Select the Firmware file for your product (fw-r10000_mmddyy.bin) 
6.	Click on upload.
7.     	The High Power Router will reboot and your page will refresh when completed.
8.    	Your firmware has now been updated.  You may disconnect your computer from the High Power Router
      	and begin using it normally.

Thank you

AMPED WIRELESS ELITE SUPPORT

___________________________________________________________________________________________________________
120712 FIRMWARE RELEASE NOTES:
- Fixed download link error.

120612 FIRMWARE RELEASE NOTES:
- Improved stability with AirPlay, AirPrint, and Home Sharing.

060812 FIRMWARE RELEASE NOTES:
- Reduced wait time between setting changes on the web interface
- Added device name for the DHCP client list

051412 FIRMWARE RELEASE NOTES:
-  Added “Allow” feature for Mac Address Filtering.  
   Users can allow only specific network devices with pre-defined Mac Addresses into the network.

120611 FIRMWARE RELEASE NOTES:
- User Interface Graphical Updates.
- Added Print button on setup summary screen. 


