AMPED WIRELESS

Model:  SR10000 Firmware Update

Firmware Version: 1.2f.08

Updated: 04/23/2012

_______________________________________________________________________________________________________


FIRMWARE UPGRADING INSTRUCTIONS:

You may call support at 888-573-8820 at anytime for questions regarding this process.

PLEASE CONNECT YOUR COMPUTER TO THE SR10000 HIGH POWER RANGE EXTENDER (REPEATER)

1.      Open your web browser and go to http://setup.ampedwireless.com 
2.      When the menu appears, click on More Settings then click Management (left side menu)
3.      Go to Upgrade Firmware.
4.      Click on choose file.
5.      Select the Firmware file for your product (fw-sr10000_mmddyy.bin) 
6.      Click on upload.
7.      The High Power Range Extender (Repeater) will reboot and your page will refresh when completed.
8.      Your firmware has now been updated.  You may disconnect your computer from the 
        High Power Range Extender (Repeater)and begin using it normally.

Thank you

AMPED WIRELESS ELITE SUPPORT

___________________________________________________________________________________________________________

042313 FIRMWARE RELEASE NOTES:
- Setup process updated to allow for Wi-Fi based setup
- Added Dashboard
- Improved User Interface

122512 FIRMWARE RELEASE NOTES:
- Fixed initial Wi-Fi network login web browser disconnect error for Apple iOS6 devices

111612 FIRMWARE RELEASE NOTES:
- Improved stability with AirPlay, AirPrint, and Home Sharing.

070312 FIRMWARE RELEASE NOTES:
- Updated web menu text and diagrams.
- Increased User Access (Mac Address Filtering) entries from 20 to 40. 
- Reduced wait time between setting changes on the web menu.

123011 FIRMWARE RELEASE NOTES:
- Fixed Home Network Connection. Now able to manually input Home Network SSID before running setup. 

121611 FIRMWARE RELEASE NOTES:
- Fixed Router Channel Change Disconnects. 
	- Range Extender (Repeater) now reconnects automatically when the Router's wireless channel changes.
	- Range Extender (Repeater) automatically reconnects in the event of a power outage or router reboot.
- Added Print button on setup summary screen. 